TightGate-Pro

Dediziertes Remote-Controlled Browser System
zum Schutz vor Gefahren aus dem Internet

Automatisch generierter Auszug aus dem Administrationshandbuch

Datum: 11.04.2019

Herausgeber:

m-privacy GmbH

Technische Redaktion

Werner-Voß-Damm 62

12101 Berlin

Fon: +49 30 243423-34

support@m-privacy.de

www.help.m-privacy.de

Allgemeine Hinweise zu diesem Handbuch

Alle Materialien und Ausführungen wurden mit Sorgfalt erarbeitet und zusammengestellt. Den­noch sind Fehler nicht auszuschließen. Die m-privacy GmbH übernimmt keine Haftung für Schäden, die aus Unrichtigkeit einzelner Angaben entstehen.

Im Sinne einer raschen Orientierung und zur Vermeidung von Sicherheitsrisiken werden besonders wichtige Aspekte durch wiederkehrende Stichworte gekennzeichnet. Diese sind:

Hinweis
Unter diesem Stichwort werden nützliche Details zur rationellen Verwendung von TightGate-Pro er­läutert.

Achtung
Unter diesem Stichwort erfolgen Hinweise zur Problemvermeidung bzw. zur Vorbeugung von Betriebs­störungen bei TightGate-Pro.

Warnung
Unter diesem Stichwort erfolgen Hinweise auf mögliche Fehler bei der Konfiguration und Verwendung von TightGate-Pro, die weitreichende Sicherheitsrisiken bergen oder zu schwerwiegenden Betriebs­störungen führen können.

Inhaltsverzeichnis

TightGate Viewer for macOS

The TightGate Viewer for macOS is available as a 64bit DMG package in the Support-Bereich the m-privacy GmbH free of charge. Supported is macOS with a version 10.8 or newer. The iOS operating system for mobile devices from Apple is currently not supported.

Installation

The available DMG package must be mounted in the directory system in the normal way (double-click). The TightGate Viewer can then be moved to the Applications directory (user authentication may be required). The TightGate viewer for macOS includes all components such as Pulseaudio for playing back audio data via TightGate-Pro.

If you are using an Apple computer with an Apple M1 chip, the Apple computer will ask you to install the Intel emulator Rosetta 2 when you start the TightGate viewer. This is necessary for Intel-based applications to run on M1 chips. Eine Instructions for Rosetta 2 from Apple can be found here.

Configuration

The setup of the TightGate viewer under macOS is done according to the convention for macOS applications. The user-specific files are located at ~/Library/Application Support/TightGate-Viewer/. The certificates generated on TightGate-Pro are also copied to this directory. The directory TightGate-Viewer must be created manually and the certificates copied there.

Firewalls or packet filters between TightGate-Pro and the Apple PC (client computer) must allow data traffic from TightGate-Pro to the Apple PC on port 4713, just like the desktop firewall on the Apple. Otherwise, no audio signals can be transmitted. If sound is activated on TightGate-Pro but the sound packets are blocked by a firewall, there will be considerable interference with video playback and use of TightGate-Pro.